­­­

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Typical** | **Non Tactile Membrane Switch** | **Membrane Switch Tactile** | **PCB Based Non Tactile** | **PCB Based Tactile** |
| **Actuation Force (g)** | 50-500 | 350-450 | 50-500 | 350-450 |
| **Switch Life** | 3 000 000 | 1 – 3 000 000 | 3 000 000 | 1 – 3 000 000 |
| **Switch Contact** | SPST Normally Open | SPST Normally Open | SPST Normally Open | SPST Normally Open |
| **Contact Rating** | 30 VDC  100 MA  1 WATT | 30 VDC  100 MA  1 WATT | 30 VDC  100 MA  1 WATT | 30 VDC  100 MA  1 WATT |
| **Contact Bounce** | <10 MS | <20 MS | <10 MS | <20 MS |
| **Contact Resistance** | <100 OHMS | <100 OHMS | <100 OHMS | <100 OHMS |
| **Capacitance** | <20 PF | <20 PF | <20 PF | <20 PF |
| **Operating Temp** | -30C-+60C | -30C-+60C | -30C-+60C | -30C-+60C |

**Generic Flexible and PCB based Membrane Keyboard Data Sheet**

Products will differ according to individual design. Please contact us to discuss your requirements.